| ActiveTcl User Guide |

## Tcl/Tk Documentation > TclCmd > read

### Tcl/Tk Applications | Tcl Commands | Tk Commands | Tcl Library | Tk Library

  NAME
    read - Read from a channel
  SYNOPSIS
    read ?-nonewline? channelId
    read channelId numChars
  DESCRIPTION
  USE WITH SERIAL PORTS
    read channelId numChars
    read channelId
  EXAMPLE
  SEE ALSO
  KEYWORDS

### NAME

read - Read from a channel

### SYNOPSIS

read ?-nonewline? channelId
read channelId numChars

### DESCRIPTION

In the first form, the read command reads all of the data from channelId up to the end of the file. If the -nonewline switch is specified then the last character of the file is discarded if it is a newline. In the second form, the extra argument specifies how many characters to read. Exactly that many characters will be read and returned, unless there are fewer than numChars left in the file; in this case all the remaining characters are returned. If the channel is configured to use a multi-byte encoding, then the number of characters read may not be the same as the number of bytes read.

ChannelId must be an identifier for an open channel such as the Tcl standard input channel (stdin), the return value from an invocation of open or socket, or the result of a channel creation command provided by a Tcl extension. The channel must have been opened for input.

If channelId is in nonblocking mode, the command may not read as many characters as requested: once all available input has been read, the command will return the data that is available rather than blocking for more input. If the channel is configured to use a multi-byte encoding, then there may actually be some bytes remaining in the internal buffers that do not form a complete character. These bytes will not be returned until a complete character is available or end-of-file is reached. The -nonewline switch is ignored if the command returns before reaching the end of the file.

Read translates end-of-line sequences in the input into newline characters according to the -translation option for the channel. See the fconfigure manual entry for a discussion on ways in which fconfigure will alter input.

### USE WITH SERIAL PORTS

For most applications a channel connected to a serial port should be configured to be nonblocking: fconfigure channelId -blocking 0. Then read behaves much like described above. Care must be taken when using read on blocking serial ports:

read channelId numChars
  In this form read blocks until numChars have been received from the serial port.
read channelId
  In this form read blocks until the reception of the end-of-file character, see fconfigure -eofchar. If there no end-of-file character has been configured for the channel, then read will block forever.

### EXAMPLE

This example code reads a file all at once, and splits it into a list, with each line in the file corresponding to an element in the list:

    set fl [open /proc/meminfo]
    set data [read $fl]
    close $fl
    set lines [split $data \n]

### SEE ALSO

file, eof, fblocked, fconfigure, Tcl_StandardChannels

### KEYWORDS

blocking, channel, end of line, end of file, nonblocking, read, translation, encoding
Copyright © 1995-1997 Roger E. Critchlow Jr. Copyright © 1993 The Regents of the University of California. Copyright © 1994-1996 Sun Microsystems, Inc.